;Model##OTHER##;Current##ELECTRICAL_CURRENT##AMPERES;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Product Documentation Link##OTHER##;Product data url##OTHER##;Product Page URL##OTHER##;Description##OTHER##;Date Created##OTHER##;Date Updated##OTHER##;Version##OTHER##;Bottle Filler 1920##OTHER##;All Connectors##OTHER##;Chiller and Grille##OTHER##;Bottle Filler 1920HO##OTHER##;1107##OTHER##;Other types##OTHER##
1107L;1107L;0;0;https://www.hawsco.com/wp-content/uploads/2020/07/haws_model_1107l_specsheet_pdf.pdf;https://www.bimobject.com/hawscorporation/product/haws-1107l;https://www.hawsco.com/products/1107l-barrier-free-wall-mount-fountain/;With internal trap allows the 1107L to be placed securely in multiple locations; 2024/03/07; 2025/10/24;2;0;0;0;0;1;0
H1107.8;H1107.8;0.23;115;https://www.hawsco.com/wp-content/uploads/2020/07/haws_model_h1107_8_specsheet_pdf.pdf;https://www.bimobject.com/hawscorporation/product/haws-h1107_8;https://www.hawsco.com/products/h1107-8-barrier-free-chilled-wall-mount-fountain/;Outfitted with such protective features as vandal-resistant bubbler head waste strainer and bottom plate; 2024/03/07; 2025/10/24;2;0;0;1;0;0;1
1107L-1920;1107L-1920;0;0;https://www.hawsco.com/wp-content/uploads/2020/07/1107l_w1920.pdf;https://www.bimobject.com/hawscorporation/product/haws-1107l-1920;https://www.hawsco.com/products/1107l-1920-ada-low-profile-wall-mount-fountain-and-bottle-filler/;Low profile barrier-free drinking fountain and bottle filler use patented stainless steel push-button activated valve assemblies allowing for front access stream adjustment as well as cartridge and strainer access; 2024/03/07; 2025/10/24;2;1;0;0;0;0;1
1107L-1920HO;1107L-1920HO;0.23;115;https://www.hawsco.com/wp-content/uploads/2021/08/1107l_w1920HO.pdf;https://www.bimobject.com/hawscorporation/product/haws-1107l-1920ho;https://www.hawsco.com/products/1107l-1920ho-ada-low-profile-wall-mount-fountain-and-touchless-bottle-filler/;Low profile barrier-free drinking fountain and bottle filler use patented stainless steel push-button activated valve assemblies allowing for front access stream adjustment as well as cartridge and strainer access; 2024/03/07; 2025/10/24;2;1;0;0;1;0;1
H1107.8-1920HO;H1107.8-1920HO;0.23;115;https://www.hawsco.com/wp-content/uploads/2021/08/h1107_8_w1920HO.pdf;https://www.bimobject.com/hawscorporation/product/haws-h1107-8-1920ho;https://www.hawsco.com/products/h1107-8-1920ho-ada-wall-mount-chilled-drinking-fountain-and-touchless-bottle-filler/;Outfitted with such protective features as vandal-resistant bubbler head waste strainer and bottom plate; 2024/03/07; 2025/10/24;2;1;0;1;1;0;1
H1107.8-1920;H1107.8-1920;0.23;115;https://www.hawsco.com/wp-content/uploads/2020/07/h1107_8_w1920.pdf;https://www.bimobject.com/hawscorporation/product/haws-h1107_8-1920;https://www.hawsco.com/products/h1107-8-1920-ada-wall-mount-drinking-fountain-and-bottle-filler/;Outfitted with such protective features as vandal-resistant bubbler head waste strainer and bottom plate; 2024/03/07; 2025/10/24;2;1;0;1;0;0;1
1107.8B;1107.8B;3.2;115;https://www.hawsco.com/wp-content/uploads/2025/06/1107.8B_specsheet.pdf;https://bimobject.com/hawscorporation/product/haws-H1107_8;https://www.hawsco.com/products/1107-8b-barrier-free-chilled-wall-mount-fountain/;Model 1107.8B, ADA vandal-resistant, wall-mounted, low-profile, 14-gauge Type 304 Stainless Steel, electric water cooler with 100% lead-free waterways. For indoor use only.; 2025/10/24; ;1;0;0;1;0;0;1
1107.8P;1107.8P;3.2;115;https://www.hawsco.com/wp-content/uploads/2020/07/h1107_8_w1920.pdf;https://bimobject.com/hawscorporation/product/haws-H1107_8-1920;https://www.hawsco.com/products/1107-8p-ada-wall-mount-drinking-fountain-and-bottle-filler/;Model 1107.8P, vandal-resistant ADA, low-profile, 14-gauge Stainless Steel electric water cooler and bottle filler, with 100% lead-free waterways. For indoor use only.; 2025/10/24; ;1;1;0;1;0;0;1
1107B;1107B;0;0;https://www.hawsco.com/wp-content/uploads/2025/06/1107B_specsheet.pdf;https://bimobject.com/hawscorporation/product/haws-1107l;https://www.hawsco.com/products/1107b-barrier-free-wall-mount-fountain/;Model 1107B, wall mounted vandal-resistant, low profile ADA, 14 gauge satin finish stainless steel drinking fountain with back panel and 100% lead free waterways.; 2025/10/24; ;1;0;0;0;0;1;0
1107P;1107P;0;0;https://www.hawsco.com/wp-content/uploads/2025/05/1107P_specsheet.pdf;https://bimobject.com/hawscorporation/product/haws-1107l-1920;https://www.hawsco.com/products/1107p-ada-low-profile-wall-mount-fountain-and-bottle-filler/;Model 1107P, wall mounted vandal-resistant, low profile ADA, 14 gauge stainless steel drinking fountain and bottle filler with 100% lead free waterways.; 2025/10/24; ;1;1;0;0;0;0;1
