;Model##OTHER##;Current##ELECTRICAL_CURRENT##AMPERES;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Product Documentation Link##OTHER##;Product data url##OTHER##;Product Page URL##OTHER##;Type Comments##OTHER##;Description##OTHER##;Date Created##OTHER##;Date Updated##OTHER##;Version##OTHER##;Bottle Filler 1920##OTHER##;All Connectors##OTHER##;1117L Geometry##OTHER##;Chiller and Grille##OTHER##;Sensor 2##OTHER##;Sensor 1##OTHER##;Bottle Filler 1920HO##OTHER##
1117LN;1117LN;0;0;https://www.hawsco.com/wp-content/uploads/2020/07/haws_model_1117ln_specsheet_pdf.pdf;https://www.bimobject.com/hawscorporation/product/haws-1117ln;https://www.hawsco.com/products/1117ln-barrier-free-dual-wall-mount-fountain/;"Hi-Lo"""" drinking fountain with antimicrobial protection* uses a patented push-button valve assembly ";"Hi-Lo"""" adjustable design allows for twice the users as regular fountains and suits the needs for various user heights"; 2024/03/07; 2025/10/24;2;0;0;0;0;0;0;0
1117LN-1920;1117LN-1920;0;0;https://www.hawsco.com/wp-content/uploads/2020/11/1117ln_w_1920a.pdf;https://www.bimobject.com/hawscorporation/product/haws-1117ln-1920;https://www.hawsco.com/products/1117ln-1920-ada-low-profile-dual-wall-mount-fountain-and-bottle-filler/;"Hi-Lo"""" drinking fountain with antimicrobial protection* uses a patented push-button valve assembly ";"""Hi-Lo"" drinking fountain and bottle filler uses patented stainless steel push-button activated valve assemblies allowing for front access stream adjustment as well as cartridge and strainer access."; 2024/03/07; 2025/10/24;2;1;0;0;0;0;0;0
1117LN-1920HO;1117LN-1920HO;0.23;115;https://www.hawsco.com/wp-content/uploads/2021/08/1117ln_w_1920HO.pdf;https://www.bimobject.com/hawscorporation/product/haws-1117ln-1920ho;https://www.hawsco.com/products/1117ln-1920ho-ada-low-profile-dual-wall-mount-fountain-and-touchless-bottle-filler/;"Hi-Lo"""" drinking fountain with antimicrobial protection* uses a patented push-button valve assembly ";"Hi-Lo"""" adjustable design allows for twice the users as regular fountains and suits the needs for various user heights"; 2024/03/07; 2025/10/24;2;1;0;0;0;0;0;1
1117L;1117L;0;0;https://www.hawsco.com/wp-content/uploads/2020/07/haws_model_1117l_specsheet_pdf.pdf;https://bimobject.com/hawscorporation/product/haws-1117l;https://www.hawsco.com/products/1117l-barrier-free-dual-wall-mount-fountain/;"""Hi-Lo"" drinking fountain with antimicrobial protection* uses a patented push-button valve assembly ";"Hi-Lo"""" adjustable design allows for twice the users as regular fountains and suits the needs for various user heights"; 2024/03/07; 2025/10/24;2;0;0;1;0;0;0;0
H1117.8-1920;H1117.8-1920;5;115;https://www.hawsco.com/wp-content/uploads/2021/01/h1117_8_w1920.pdf;https://www.bimobject.com/hawscorporation/product/h11178-1920;https://www.hawsco.com/products/h1117-8-1920/;"""Hi-Lo"" electric drinking fountain with antimicrobial protection* provides 8 gph chilled water performance in an engineered stainless steel skin";Designed to run at a low energy usage this water cooler and fountain are assured to have a long lasting life; 2024/03/07; 2025/10/24;2;1;0;1;1;0;0;0
H1117.8-1920HO;H1117.8-1920HO;5;115;https://www.hawsco.com/wp-content/uploads/2024/06/H1117.8-1920HO_specsheet.pdf;https://www.bimobject.com/en-us/hawscorporation/product/h11178-1920ho;https://www.hawsco.com/products/h1117-8-1920ho-ada-vandal-resistant-chilled-adjustable-drinking-fountain-and-motion-activated-bottle-filler/;"""Hi-Lo"" electric drinking fountain with antimicrobial protection* provides 8 gph chilled water performance in an engineered stainless steel skin";Designed to run at a low energy usage this water cooler and fountain are assured to have a long lasting life; 2024/03/07; 2025/10/24;2;1;0;1;1;0;0;1
1117B;1117B;0;0;https://www.hawsco.com/wp-content/uploads/2025/05/1117B_specsheet.pdf;https://bimobject.com/hawscorporation/product/haws-1117LN;https://www.hawsco.com/products/1117b-ada-vandal-resistant-wall-mount-drinking-fountain/;"Hi-Lo"""" drinking fountain with antimicrobial protection* uses a patented push-button valve assembly ";Model 1117B, Hi-Lo ADA, wall mounted vandal-resistant, dual 14 gauge satin finish stainless steel drinking fountain with back panel and 100% lead free waterways.; 2025/10/24; ;1;0;0;0;0;0;0;0
1117P;1117P;0;0;https://www.hawsco.com/wp-content/uploads/2020/11/1117ln_w_1920a.pdf;https://bimobject.com/hawscorporation/product/haws-1117LN-1920;https://www.hawsco.com/products/1117p-ada-low-profile-dual-wall-mount-fountain-and-bottle-filler/;"Hi-Lo"""" drinking fountain with antimicrobial protection* uses a patented push-button valve assembly ";Model 1117P, Hi-Lo, ADA wall mounted vandal-resistant, dual 14 gauge satin finish stainless steel drinking fountain and bottle filler.; 2025/10/24; ;1;1;0;0;0;0;0;0
H1117.8;H1117.8;0;0;https://www.hawsco.com/wp-content/uploads/2021/07/H1117LN.8spec.pdf;https://bimobject.com/hawscorporation/product/haws-1117_8;https://www.hawsco.com/products/h1117-8-barrier-free-chilled-dual-wall-mount-fountain/;"Hi-Lo"""" drinking fountain with antimicrobial protection* uses a patented push-button valve assembly ";Designed to run at a low energy usage, this water cooler and fountain are assured to have a long lasting life; 2014/03/24; 2025/10/28;2;0;0;1;1;0;0;0
H1117.8HO;H1117.8HO;5;115;https://www.hawsco.com/wp-content/uploads/2021/07/H1117LN.8spec.pdf;https://www.bimobject.com/hawscorporation/product/haws-h1117_8ho;https://www.hawsco.com/products/h1117-8ho-chilled-wall-mount-ada-touchless-push-button-dual-adjustable-fountain/;Hi-Lo electric drinking fountain with antimicrobial protection* provides 8 gph chilled water performance in an engineered stainless steel skin;Designed to run at a low energy usage, this water cooler and fountain are assured to have a long lasting life; 2014/03/24; 2025/10/28;2;0;0;1;1;0;1;0
H1117.8HO2;H1117.8HO2;5;115;https://www.hawsco.com/wp-content/uploads/2021/07/H1117LN.8spec.pdf;https://www.bimobject.com/hawscorporation/product/haws-h1117_8ho2;https://www.hawsco.com/products/h1117-8ho2-chilled-wall-mount-ada-touchless-dual-adjustable-fountain/;Hi-Lo electric drinking fountain with antimicrobial protection* provides 8 gph chilled water performance in an engineered stainless steel skin;Designed to run at a low energy usage, this water cooler and fountain are assured to have a long lasting life; 2014/03/24; 2025/10/28;2;0;0;1;1;1;1;0
1117.8B;1117.8B;3.2;115;https://www.hawsco.com/wp-content/uploads/2025/05/1117.8B_specsheet.pdf;https://bimobject.com/hawscorporation/product/1117-8b-ada-low-profile-dual-chilled-vandal-resistant-fountain;https://www.hawsco.com/products/1117-8b-ada-low-profile-dual-chilled-vandal-resistant-fountain/;"Hi-Lo"""" drinking fountain with antimicrobial protection* uses a patented push-button valve assembly ";Model 1117.8B, ADA vandal-resistant, wall mounted 14 gauge dual fountain satin finish stainless steel electric water cooler with back panel and 100% lead free waterways. For indoor use only.; 2025/10/28; ;1;0;0;0;1;0;0;0
1117.8P;1117.8P;3.2;115;https://www.hawsco.com/wp-content/uploads/2021/06/H1117LN.8-1920spec.pdf;https://bimobject.com/hawscorporation/product/1117-8p-ada-low-profile-dual-chilled-vandal-resistant-fountain;https://www.hawsco.com/products/1117-8p-ada-low-profile-dual-chilled-vandal-resistant-fountain/;"Hi-Lo"""" drinking fountain with antimicrobial protection* uses a patented push-button valve assembly ";Model 1117.8P, ADA vandal-resistant, wall mounted 14 gauge dual fountain satin finish stainless steel electric water cooler and bottle filler with back panel and 100% lead free waterways. For indoor use only.; 2025/10/28; ;1;1;0;0;1;0;0;0
